# Irrigation efficiency

Season
Field
Metric

##### Efficiency by field

##### Summary

- Average application efficiency: 84%.
- Estimated water saved vs baseline: 24%.
- South Vegetables below target—investigate emitter uniformity.
- Greenhouse 1 performing at high efficiency.

##### Field efficiency details

Field | Application efficiency | Distribution uniformity | Notes
--- | --- | --- | ---
North Orchard | 86% | 0.81 | Within target; maintain current settings.
South Vegetables | 76% | 0.72 | Check leaks and emitter clogging; consider redesign in SV-03.
West Maize | 83% | 0.78 | Efficiency drops during heat waves; review schedule timing.
Greenhouse 1 | 92% | 0.88 | Best performer; use as reference configuration.